#title GetJointMotorForce [RCBasic Doc]
#header Function  GetJointMotorForce( joint_id,   inv_dt)

Return the current motor force given the inverse time step, usually in N. 

Used with Prismatic Joint

#ref SetJointMotorForce

